All ies and ldt files for fixtures with LED71TW-5020 modules are tested at 5000K.
Factors to adjust lumen output for the following CCTs at 100% output for the colour are as follows:

@ 2000K - x0.75
@ 2700K - x0.93
@ 3500K - x1.07
@ 4000K - x1.11
@ 5000K - x1.17


